**Last data updates: 27 March 2013**

Zhang, L., Hong, S., He, J., Gan, F.X. and Ho, Y.S. (2010), Isotherm study of phosphorus uptake from aqueous solution using aluminum oxide. *Clean-Soil Air Water*, **38** (9), 831-836.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Document type: Article | Language: English | Cited references: 17 | Times cited: 5 | Times self cited: 0 |

Abstract: Aluminum oxide, which could be an alternative filter media for phosphorus uptake from aqueous solution, was selected as an adsorbent for the isotherm study of phosphorus uptake from aqueous solution. Batch method was adopted to investigate the adsorption behavior of phosphorus onto aluminum oxide. The Langmuir, Freundlich, and Redlich-Peterson isotherms were used to analyze the experimental data by both the linear and nonlinear regression methods. The adsorption experiment was conducted at various temperatures, to choose the appropriate method and obtain the creditable adsorption parameters for phosphorus uptake studies. The results indicated that the nonlinear regression method might be a better way to compare the best-fitting isotherm and obtain the parameters for the adsorption of phosphorus onto aluminum oxide. Both the Redlich-Peterson and the Freundlich isotherms have high coefficients of determination for the adsorption of phosphorus onto aluminum oxide at various temperatures. In addition, a new relationship between the Redlich-Peterson and the Freundlich isotherm parameters was presented.

Author Keywords: Adsorption; Aluminum oxide; Isotherm parameters; Nonlinear regression; Phosphorus

KeyWords Plus: Sorption Isotherm; Adsorption; Gases

Reprint Address: Ho, YS (reprint author), Asia Univ, Water Res Ctr, 500 Lioufeng Rd, Taichung 41354, Taiwan

Addresses:

1. Asia Univ, Water Res Ctr, Taichung 41354, Taiwan

2. Chinese Acad Sci, Inst Geodesy & Geophys, Wuhan, Peoples R China

3. Wuhan Univ, Sch Resource & Environm Sci, Wuhan 430072, Peoples R China

4. China Med Univ, Dept Publ Hlth, Taichung, Taiwan

E-mail Addresses: [ysho@asia.edu.tw](mailto:ysho@asia.edu.tw)

1. Sun, J.N., Xu, G., Shao, H.B. and Xu, S.H. (2012), Potential Retention and Release Capacity of Phosphorus in the Newly Formed Wetland Soils from the Yellow River Delta, China. *Clean-Soil Air Water*, **40** (10), 1131-1136.
2. Choi, J.W., Lee, S.Y., Lee, S.H., Kim, J.E., Park, K.Y., Kim, D.J. and Hong, S.W. (2012), Comparison of Surface-Modified Adsorbents for Phosphate Removal in Water. *Water Air and Soil Pollution*, **223** (6), 2881-2890.
3. Choi, J.W., Lee, S.Y., Lee, S.H., Lee, K.B., Kim, D.J. and Hong, S.W. (2012), Adsorption of Phosphate by Amino-Functionalized and Co-condensed SBA-15. *Water Air and Soil Pollution*, **223** (5), 2551-2562.
4. Choi, J.W., Chung, S.G., Baek, K.Y., Cho, K.Y., Hong, S.W., Kim, D.J. and Lee, S.H. (2012), Removal of Benzene Using the Characteristics of Block Copolymers for Encapsulation. *Water Air and Soil Pollution* , **223** (2), 609-616.
5. Kizilkaya, B. and Tekinay, A.A. (2011), Comparative Study and Removal of Co and Ni (II) Ions from Aqueous Solutions Using Fish Bones. *Science of Advanced Materials*, **3** (6), 949-961.