**Last data updates: 25 January 2012**

Ho, Y.S.\* (2011), Comment on “comparison of two-stage sorption design models for the removal of lead ions by polyvinyl-modified Kaolinite clay”. *Journal of Hazardous Materials*, **198** (1), 387.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Document type: Letter | Language: English | Cited references: 9 | Times cited: 0 | Times self cited: 0 |

KeyWords Plus: Pseudo-Isotherms; Kinetic-Model; Peat; Dye

Reprint Address: Ho, YS (reprint author), Asia Univ, Water Res Ctr, Taichung 41354, Taiwan

Addresses:

1. Asia Univ, Water Res Ctr, Taichung 41354, Taiwan

E-mail Address: ysho@asia.edu.tw