**Last data updates: 07 December 2015**

Ho, Y.S. (1995), Adsorption of heavy metals from waste streams by peat. *Ph.D. Thesis*, University of Birmingham, Birmingham, U.K.

Times cited: 331

1. Ho, Y.S. (2015), Comment on “Genetic characterization, nickel tolerance, biosorption, kinetics, and uptake mechanism of a bacterium isolated from electroplating industrial effluent”. *Canadian Journal of Microbiology*, **61** (11), 881-882.
2. Kwon, J.H., Wilson, L.D. and Sammynaiken, R. (2015), Sorptive uptake of selenium with magnetite and its supported materials onto activated carbon. *Journal of Colloid and Interface Science*, **457**), 388-397.
3. Balaz, M., Bujnakova, Z., Balaz, P., Zorkovska, A., Dankova, Z. and Briancin, J. (2015), Adsorption of cadmium(II) on waste biomaterial. *Journal of Colloid and Interface Science*, **454**), 121-133.
4. Mahmoodi, N.M. and Masrouri, O. (2015), Cationic Dye Removal Ability from Multicomponent System by Magnetic Carbon Nanotubes. *Journal of Solution Chemistry*, **44** (8), 1568-1583.
5. Liu, S.J. (2015), Cooperative adsorption on solid surfaces. *Journal of Colloid and Interface Science*, **450**), 224-238.
6. Ho, Y.S. (2015), Comments on “Isothermic and Kinetic Modeling of Fluoride Removal from Water by Means of the Natural Biosorbents Sorghum and Canola”. *Fluoride*, **48** (3), 266-268.
7. Jia, A.Y., Wu, C.D., Hu, W.C. and Hu, C.X. (2015), Bromate Adsorption on Three Variable Charge Soils: Kinetics and Thermodynamics. *Clean-Soil Air Water*, **43** (7), 1072-1077.
8. Santos, S.C.R. and Boaventura, R.A.R. (2015), Treatment of a simulated textile wastewater in a sequencing batch reactor (SBR) with addition of a low-cost adsorbent. *Journal of Hazardous Materials*, **291**), 74-82.
9. Mahmoodi, N.M. and Ghobadi, J. (2015), Extended isotherm and kinetics of binary system dye removal using carbon nanotube from wastewater. *Desalination and Water Treatment*, **54** (10), 2777-2793.
10. Liu, S.J. (2015), A mathematical model for competitive adsorptions. *Separation and Purification Technology*, **144**), 80-89.
11. Mahmoodi, N.M. and Maghsoodi, A. (2015), Kinetics and isotherm of cationic dye removal from multicomponent system using the synthesized silica nanoparticle. *Desalination and Water Treatment*, **54** (2), 562-571.
12. Ho, Y.S. (2015), Comments on “Synthesis and Adsorption of Ni(II) on Ni(II)-Imprinted Polyaniline Supported on Attapulgite Modified with 3-Methacryloxypropyltrimethoxysilane”. *Adsorption Science & Technology*, **33** (4), 427-428.
13. Mariappan, R., Vairamuthu, R. and Ganapathy, A. (2015), Use of chemically activated cotton nut shell carbon for the removal of fluoride contaminated drinking water: Kinetics evaluation. *Chinese Journal of Chemical Engineering*, **23** (4), 710-721.
14. Zhao, J.M., Hu, Q.Y., Li, Y.B. and Liu, H.Z. (2015), Efficient separation of vanadium from chromium by a novel ionic liquid-based synergistic extraction strategy. *Chemical Engineering Journal*, **264**), 487-496.
15. Bhatt, R., Sreedhar, B. and Padmaja, P. (2015), Adsorption of chromium from aqueous solutions using crosslinked chitosan-diethylenetriaminepentaacetic acid. *International Journal of Biological Macromolecules*, **74**), 458-466.
16. Olajire, A.A., Giwa, A.A. and Bello, I.A. (2015), Competitive adsorption of dye species from aqueous solution onto melon husk in single and ternary dye systems. *International Journal of Environmental Science and Technology*, **12** (3), 939-950.
17. Ghaedi, M., Ansari, A., Bahari, F., Ghaedi, A.M. and Vafaei, A. (2015), A hybrid artificial neural network and particle swarm optimization for prediction of removal of hazardous dye brilliant green from aqueous solution using zinc sulfide nanoparticle loaded on activated carbon. *Spectrochimica Acta Part A-Molecular and Biomolecular Spectroscopy*, **137**), 1004-1015.
18. Tiwari, D., Lalhmunsiama and Lee, S.M. (2015), Iron-impregnated activated carbons precursor to rice hulls and areca nut waste in the remediation of Cu(II) and Pb(II) contaminated waters: a physico-chemical studies. *Desalination and Water Treatment*, **53** (6), 1591-1605.
19. Su, Y., Liu, J., Yue, Q.Y., Li, Q. and Gao, B.Y. (2015), Adsorption of Lead and Nickel Ions by Semi-interpenetrating Network Hydrogel Based on Wheat Straw Cellulose: Kinetics, Equilibrium, and Thermodynamics. *Soft Materials*, **13** (4), 225-236.
20. Rahman, M.S. and Sathasivam, K.V. (2015), Heavy Metal Adsorption onto Kappaphycus sp from Aqueous Solutions: The Use of Error Functions for Validation of Isotherm and Kinetics Models. *Biomed Research International*, .
21. Zhu, M.H., Zhao, J.M., Li, Y.B., Mehio, N., Qi, Y.R., Liu, H.Z. and Dai, S. (2015), An ionic liquid-based synergistic extraction strategy for rare earths. *Green Chemistry*, **17** (5), 2981-2993.
22. Zhou, C.Q., Gong, X.X., Han, J. and Guo, R. (2015), Controlled synthesis of tower-like aniline oligomers with excellent adsorption properties. *New Journal of Chemistry*, **39** (3), 2202-2208.
23. Hammud, H.H., Shmait, A. and Hourani, N. (2015), Removal of Malachite Green from water using hydrothermally carbonized pine needles. *Rsc Advances*, **5** (11), 7909-7920.
24. Mahdavi, S., Jalali, M. and Afkhami, A. (2015), Heavy metals removal from aqueous solutions by Al2O3 nanoparticles modified with natural and chemical modifiers. *Clean Technologies and Environmental Policy* , **17** (1), 85-102.
25. Wang, F.C., Zhao, J.M., Zhu, M.H., Yu, J.Z., Hu, Y.S. and Liu, H.Z. (2015), Selective adsorption-deposition of gold nanoparticles onto monodispersed hydrothermal carbon spherules: a reduction-deposition coupled mechanism. *Journal of Materials Chemistry A*, **3** (4), 1666-1674.
26. Wang, M.X., Zhang, Q.L. and Yao, S.J. (2015), A novel biosorbent formed of marine-derived Penicillium janthinellum mycelial pellets for removing dyes from dye-containing wastewater. *Chemical Engineering Journal*, **259**), 837-844.
27. Mahmoodi, N.M., Maghsoudi, A., Najafi, F., Jalili, M. and Kharrati, H. (2014), Primary-secondary amino silica nanoparticle: synthesis and dye removal from binary system. *Desalination and Water Treatment*, **52** (40-42), 7784-7796.
28. Ho, Y.S. (2014), Comments on “Adsorption of 2-mercaptobenzothiazole from aqueous solution by organo-bentonite” by P. Jing, MH Hou, P. Zhao, XY Tang, HF Wan. *Journal of Environmental Sciences-China*, **26** (12), 2571-2572.
29. Tiwari, D., Lalhmunsiama, Choi, S.I. and Lee, S.M. (2014), Activated Sericite: An Efficient and Effective Natural Clay Material for Attenuation of Cesium from Aquatic Environment. *Pedosphere*, **24** (6), 731-742.
30. Ho, Y.S. (2014), Comments on “Simultaneous Adsorption of Aniline and Cr(VI) Ion by Activated Carbon/Chitosan Composite”. *Journal of Applied Polymer Science*, **131** (22.
31. Wang, Q., Zhang, D.H., Tian, S.L. and Ning, P. (2014), Simultaneous Adsorptive Removal of Methylene Blue and Copper Ions from Aqueous Solution by Ferrocene-Modified Cation Exchange Resin. *Journal of Applied Polymer Science*, **131** (21.
32. Dutta, D.P., Singh, A., Ballal, A. and Tyagi, A.K. (2014), High Adsorption Capacity for Cationic Dye Removal and Antibacterial Properties of Sonochemically Synthesized Ag2WO4 Nanorods. *European Journal of Inorganic Chemistry*, (33), 5724-5732.
33. Ho, Y.S. (2014), Affinity adsorption of lysozyme with Reactive Red 120-modified magnetic chitosan microspheres. *Food Chemistry*, **161**), 323.
34. Krishni, R.R., Foo, K.Y. and Hameed, B.H. (2014), Adsorption of cationic dye using a low-cost biowaste adsorbent: equilibrium, kinetic, and thermodynamic study. *Desalination and Water Treatment*, **52** (31-33), 6088-6095.
35. Xing, G.X., Liu, S.L., Tang, Y.F., Jiang, H. and Liu, Q.W. (2014), Preparation of cationic functional starch/Na+-MMT composite and its application for effective removal of three hazardous metal anionic ions with different valence. *Starch-Starke*, **66** (9-10), 824-831.
36. Mishra, P.C., Islam, M. and Patel, R.K. (2014), Removal of nitrate-nitrogen from aqueous medium by adsorbents derived from pomegranate rind. *Desalination and Water Treatment*, **52** (28-30), 5673-5680.
37. Mahmoodi, N.M., Banijamali, M. and Noroozi, B. (2014), Surface Modification and Ternary System Dye Removal Ability of Manganese Ferrite Nanoparticle. *Fibers and Polymers*, **15** (8), 1616-1626.
38. Mahmoodi, N.M., Masrouri, O. and Najafi, F. (2014), Dye Removal Using Polymeric Adsorbent from Wastewater Containing Mixture of Two Dyes. *Fibers and Polymers*, **15** (8), 1656-1668.
39. Ofomaja, A.E., Pholosi, A. and Naidoo, E.B. (2014), Kinetics and competitive modeling of cesium biosorption onto iron(III) hexacyanoferrate modified pine cone powder. *International Biodeterioration & Biodegradation*, **92**), 71-78.
40. Mahmoodi, N.M., Masrouri, O. and Najafi, F. (2014), Synthesis of urethane sodium carboxylate and its dye removal ability from single system. *Journal of Industrial and Engineering Chemistry*, **20** (4), 1558-1565.
41. Ghaedi, M., Ghaedi, A.M., Hossainpour, M., Ansari, A., Habibi, M.H. and Asghari, A.R. (2014), Least square-support vector (LS-SVM) method for modeling of methylene blue dye adsorption using copper oxide loaded on activated carbon: Kinetic and isotherm study. *Journal of Industrial and Engineering Chemistry*, **20** (4), 1641-1649.
42. Mahmoodi, N.M. (2014), Synthesis of core-shell magnetic adsorbent nanoparticle and selectivity analysis for binary system dye removal. *Journal of Industrial and Engineering Chemistry*, **20** (4), 2050-2058.
43. Mahmoodi, N.M., Masrouri, O. and Arabi, A.M. (2014), Synthesis of porous adsorbent using microwave assisted combustion method and dye removal. *Journal of Alloys and Compounds*, **602**), 210-220.
44. Hu, Q.Y., Paudyal, H., Zhao, J.M., Huo, F., Inoue, K. and Liu, H.Z. (2014), Adsorptive recovery of vanadium(V) from chromium(VI)-containing effluent by Zr(IV)-loaded orange juice residue. *Chemical Engineering Journal*, **248**), 79-88.
45. Hu, X.J., Liu, Y.G., Zeng, G.M., Wang, H., Hu, X., Chen, A.W., Wang, Y.Q., Guo, Y.M., Li, T.T., Zhou, L., Liu, S.H. and Zeng, X.X. (2014), Effect of aniline on cadmium adsorption by sulfanilic acid-grafted magnetic graphene oxide sheets. *Journal of Colloid and Interface Science*, **426**), 213-220.
46. Mahmoodi, N.M. (2014), Dendrimer functionalized nanoarchitecture: Synthesis and binary system dye removal. *Journal of the Taiwan Institute of Chemical Engineers*, **45** (4), 2008-2020.
47. Ho, Y.S. (2014), Comments on “Elimination of Bisphenol A from Water via Graphene Oxide Adsorption”. *Acta Physico-Chimica Sinica*, **30** (7), 1391.
48. Wang, F.C., Zhao, J.M., Wei, X.T., Huo, F., Li, W.S., Hu, Q.Y. and Liu, H.Z. (2014), Adsorption of rare earths (III) by calcium alginate-poly glutamic acid hybrid gels. *Journal of Chemical Technology and Biotechnology*, **89** (7), 969-977.
49. Ho, Y.S. (2014), Comment on “New Calix[4]arene Appended Amberlite XAD-4 Resin with Versatile Perchlorate Removal Efficiency”. *Journal of Chemical and Engineering Data*, **59** (6), 2131.
50. Ho, Y.S. (2014), Using of “pseudo-second-order model” in adsorption. *Environmental Science and Pollution Research*, **21** (11), 7234-7235.
51. Spiridon, O.B. and Pitulice, L. (2014), Response to “Using of ‘pseudo-second-order model’ in adsorption”, comment letter on “Phenol removal from wastewater by adsorption on zeolitic composite” [Bizerea Spiridon et al., Environ Sci Pollut Res (2013) 20:6367-6381]. *Environmental Science and Pollution Research*, **21** (11), 7236-7237.
52. Soni, H. and Padmaja, P. (2014), Palm shell based activated carbon for removal of bisphenol A: an equilibrium, kinetic and thermodynamic study. *Journal of Porous Materials*, **21** (3), 275-284.
53. Ho, Y.S. (2014), Comments on “Adsorption characteristics and behaviors of graphene oxide for Zn(II) removal from aqueous solution”. *Applied Surface Science*, **301**), 584.
54. Yan, Y.B., Sun, X.Y., Ma, F.B., Li, J.S., Shen, J.Y., Han, W.Q., Liu, X.D. and Wang, L.J. (2014), Removal of phosphate from wastewater using alkaline residue. *Journal of Environmental Sciences-China*, **26** (5), 970-980.
55. Hackbarth, F.V., Vilar, V.J.P., De Souza, G.B., de Souza, S.M.A.G. and de Souza, A.A.U. (2014), Benzene, toluene and o-xylene (BTX) removal from aqueous solutions through adsorptive processes. *Adsorption-Journal of the International Adsorption Society*, **20** (4), 577-590.
56. Kwon, J.H., Wilson, L.D. and Sammynaiken, R. (2014), Sorptive Uptake Studies of an Aryl-Arsenical with Iron Oxide Composites on an Activated Carbon Support. *Materials*, **7** (3), 1880-1898.
57. Mahmoodi, N.M., Abdi, J. and Najafi, F. (2014), Synthesis of Urethane Polycarboxylate as a Novel Adsorbent and Its Binary System Dye Removal Ability from Aqueous Solution. *Fibers and Polymers*, **15** (3), 446-456.
58. Lee, S.M., Lalhmunsiama and Tiwari, D. (2014), Sericite in the remediation of Cd(II)- and Mn(II)-contaminated waters: batch and column studies. *Environmental Science and Pollution Research*, **21** (5), 3686-3696.
59. Tseng, R.L., Wu, P.H., Wu, F.C. and Juang, R.S. (2014), A convenient method to determine kinetic parameters of adsorption processes by nonlinear regression of pseudo-nth-order equation. *Chemical Engineering Journal*, **237**), 153-161.
60. Moradi, S.E. (2014), Microwave assisted preparation of sodium dodecyl sulphate (SDS) modified ordered nanoporous carbon and its adsorption for MB dye. *Journal of Industrial and Engineering Chemistry*, **20** (1), 208-215.
61. Abdelwahab, O., Amin, N.K. and El-Ashtoukhy, E.S.Z. (2014), The Investigation of Phenol Removal from Aqueous Solutions by Water Hyacinth. *Separation Science and Technology*, **49** (10), 1604-1612.
62. Murithi, G., Onindo, C.O., Wambu, E.W. and Muthakia, G.K. (2014), Removal of Cadmium(II) Ions from Water by Adsorption using Water Hyacinth (Eichhornia crassipes) Biomass. *Bioresources*, **9** (2), 3613-3631.
63. Ho, Y.S. (2014), The real pseudo-second-order rate equation. *Industrial Crops and Products*, **52**), 17.
64. Dahlan, I. and Noor, A.S.M. (2014), Study on the Removal Characteristic of Acid Violet Dye from Synthetic Wastewater Using A Novel Rha/Pfa/Cfa Sorbent. *Environmental Engineering and Management Journal*, **13** (1), 197-204.
65. Ofomaja, A.E., Pholosi, A. and Naidoo, E.B. (2013), Kinetics and competitive modeling of cesium biosortion onto chemically modified pine cone powder. *Journal of the Taiwan Institute of Chemical Engineers*, **44** (6), 943-951.
66. Mahmoodi, N.M. (2013), Synthesis of Amine-Functionalized Magnetic Ferrite Nanoparticle and Its Dye Removal Ability. *Journal of Environmental Engineering*, **139** (11), 1382-1390.
67. Ong, S.A., Ho, L.N., Wong, Y.S. and Zainuddin, A. (2013), Adsorption Behavior of Cationic and Anionic Dyes onto Acid Treated Coconut Coir. *Separation Science and Technology*, **48** (14), 2125-2131.
68. Song, S.T., Saman, N., Johari, K. and Mat, H. (2013), Removal of Hg(II) from Aqueous Solution by Adsorption Using Raw and Chemically Modified Rice Straw As Novel Adsorbents. *Industrial & Engineering Chemistry Research*, **52** (36), 13092-13101.
69. Wang, J., Liu, P., Li, Z., Qi, W., Lu, Y. and Wu, W.S. (2013), Th(IV) Adsorption onto Oxidized Multi-Walled Carbon Nanotubes in the Presence of Hydroxylated Fullerene and Carboxylated Fullerene. *Materials* , **6** (9), 4168-4185.
70. Ho, Y.S. (2013), Comments on “Removal of zirconium(IV) from aqueous solution by Coriolus versicolor: Equilibrium and thermodynamic study”. *Ecological Engineering*, **58**), 1-2.
71. Wang, F.C., Zhao, J.M., Li, W.S., Zhou, H.C., Yang, X.F., Sui, N. and Liu, H.H. (2013), Preparation of Several Alginate Matrix Gel Beads and their Adsorption Properties Towards Rare Earths (III). *Waste and Biomass Valorization*, **4** (3), 665-674.
72. Wang, J., Li, Z., Li, S.C., Qi, W., Liu, P., Liu, F.Q., Ye, Y.L., Wu, L.S., Wang, L. and Wu, W.S. (2013), Adsorption of Cu(II) on Oxidized Multi-Walled Carbon Nanotubes in the Presence of Hydroxylated and Carboxylated Fullerenes. *Plos One*, **8** (8.
73. Zhao, D.L., Ding, Y., Chen, S.H., Zhang, K.H. and Liu, C. (2013), Kinetics of the Sorption of Cobalt Onto Mg/Al Layered Double Hydroxide. *Asian Journal of Chemistry*, **25** (10), 5713-5715.
74. Zhao, D.L., Ding, Y., Chen, S.H., Bai, T.T. and Ma, Y.L. (2013), Adsorption of Methylene Blue on Carbon Nanotubes from Aqueous Solutions. *Asian Journal of Chemistry*, **25** (10), 5756-5758.
75. Li, J., Chen, C.L., Zhao, Y., Hu, J., Shao, D.D. and Wang, X.K. (2013), Synthesis of water-dispersible Fe3O4@beta-cyclodextrin by plasma-induced grafting technique for pollutant treatment. *Chemical Engineering Journal*, **229**), 296-303.
76. Li, B.Z., Sun, K.Q., Guo, Y.B., Tian, J.P., Xue, Y.B. and Sun, D.K. (2013), Adsorption kinetics of phenol from water on Fe/AC. *Fuel*, **110**), 99-106.
77. Mahmoodi, N.M., Abdi, J. and Najafi, F. (2013), Gemini polymeric nanoarchitecture as a novel adsorbent: Synthesis and dye removal from multicomponent system. *Journal of Colloid and Interface Science*, **400**), 88-96.
78. Zafar, M.N., Parveen, A. and Nadeem, R. (2013), A pretreated green biosorbent based on Neem leaves biomass for the removal of lead from wastewater. *Desalination and Water Treatment*, **51** (22-24), 4459-4466.
79. Roy, A., Adhikari, B. and Majumder, S.B. (2013), Equilibrium, Kinetic, and Thermodynamic Studies of Azo Dye Adsorption from Aqueous Solution by Chemically Modified Lignocellulosic Jute Fiber. *Industrial & Engineering Chemistry Research*, **52** (19), 6502-6512.
80. Foo, K.Y., Lee, L.K. and Hameed, B.H. (2013), Preparation of banana frond activated carbon by microwave induced activation for the removal of boron and total iron from landfill leachate. *Chemical Engineering Journal*, **223**), 604-610.
81. Foo, K.Y., Lee, L.K. and Hameed, B.H. (2013), Batch adsorption of semi-aerobic landfill leachate by granular activated carbon prepared by microwave heating. *Chemical Engineering Journal*, **222**), 259-264.
82. Guo, L., Li, G.Y., Liu, J.S., Meng, Y.F. and Tang, Y.F. (2013), Adsorptive decolorization of methylene blue by crosslinked porous starch. *Carbohydrate Polymers*, **93** (2), 374-379.
83. Foo, K.Y., Lee, L.K. and Hameed, B.H. (2013), Preparation of activated carbon from sugarcane bagasse by microwave assisted activation for the remediation of semi-aerobic landfill leachate. *Bioresource Technology*, **134**), 166-172.
84. Wang, F.C., Zhao, J.M., Pan, F., Zhou, H.C., Yang, X.F., Li, W.S. and Liu, H.Z. (2013), Adsorption Properties toward Trivalent Rare Earths by Alginate Beads Doping with Silica. *Industrial & Engineering Chemistry Research*, **52** (9), 3453-3461.
85. Zafar, M.N., Wahid, A., Ghauri, M.A., Zubair, M., Mumtaz, M.W., Anwar, F. and Danish, M. (2013), Trichoderma harzianum: a green sorbent for Pb(II) uptake from aqueous solutions. *Toxicological and Environmental Chemistry*, **95** (3), 422-433.
86. Chandra, I.K., Ju, Y.H., Ayucitra, A. and Ismadji, S. (2013), Evans blue removal from wastewater by rarasaponin-bentonite. *International Journal of Environmental Science and Technology*, **10** (2), 359-370.
87. Mahmoodi, N.M., Najafi, F. and Neshat, A. (2013), Poly (amidoamine-co-acrylic acid) copolymer: Synthesis, characterization and dye removal ability. *Industrial Crops and Products*, **42**), 119-125.
88. Sadeghi-Kiakhani, M., Arami, M. and Gharanjig, K. (2013), Dye Removal from Colored-Textile Wastewater Using Chitosan-PPI Dendrimer Hybrid as a Biopolymer: Optimization, Kinetic, and Isotherm Studies. *Journal of Applied Polymer Science*, **127** (4), 2607-2619.
89. Foo, K.Y. and Hameed, B.H. (2013), Utilization of oil palm biodiesel solid residue as renewable sources for preparation of granular activated carbon by microwave induced KOH activation. *Bioresource Technology*, **130**), 696-702.
90. Mahmoodi, N.M. (2013), Nickel Ferrite Nanoparticle: Synthesis, Modification by Surfactant and Dye Removal Ability. *Water Air and Soil Pollution*, **224** (2.
91. Raj, K.R., Kardam, A., Arora, J.K., Srivastava, S. and Srivastava, M.M. (2013), Adsorption behavior of dyes from aqueous solution using agricultural waste: modeling approach. *Clean Technologies and Environmental Policy*, **15** (1), 73-80.
92. Wang, F.C., Zhao, J.M., Zhou, H.C., Li, W.S., Sui, N. and Liu, H.Z. (2013), O-carboxymethyl chitosan entrapped by silica: preparation and adsorption behaviour toward neodymium (III) ions. *Journal of Chemical Technology and Biotechnology*, **88** (2), 317-325.
93. Zhao, D.L., Wang, Y., Xuan, H., Chen, Y. and Cao, T. (2013), Removal of radiocobalt from aqueous solution by Mg2Al layered double hydroxide. *Journal of Radioanalytical and Nuclear Chemistry*, **295** (2), 1251-1259.
94. Wang, H.L., Huang, Y., Wang, Q., Zhai, L.F. and Jiang, S.T. (2013), Residue Resulted after Wheat Bran Fermentation with Aspergillus niger Sorption Behavior of Cobalt as a Function of Environmental Conditions. *Industrial & Engineering Chemistry Research*, **52** (3), 1352-1358.
95. Ai, L.H. and Zeng, Y. (2013), Hierarchical porous NiO architectures as highly recyclable adsorbents for effective removal of organic dye from aqueous solution. *Chemical Engineering Journal*,  **215**), 269-278.
96. Njoku, V.O., Foo, K.Y. and Hameed, B.H. (2013), Microwave-assisted preparation of pumpkin seed hull activated carbon and its application for the adsorptive removal of 2,4-dichlorophenoxyacetic acid. *Chemical Engineering Journal*, **215**), 383-388.
97. Korkmaz, M., Ozmetin, C., Fil, B.A., Ozmetin, E. and Yasar, Y. (2013), Methyl Violet Dye Adsorption Onto Clinoptilolite (Natural Zeolite): Isotherm and Kinetic Study. *Fresenius Environmental Bulletin*, **22** (5A), 1524-1533.
98. Zhang, D.Y., Lee, D.J. and Pan, X.L. (2013), Desorption of Hg(II) and Sb(V) on extracellular polymeric substances: Effects of pH, EDTA, Ca(II) and temperature shocks. *Bioresource Technology*, **128**), 711-715.
99. Moradi, O. and Zare, K. (2013), Adsorption of Ammonium Ion by Multi-walled Carbon Nanotube: Kinetics and Thermodynamic Studies. *Fullerenes Nanotubes and Carbon Nanostructures*, **21** (6), 449-459.
100. Burnett, J.L., Croudace, I.W. and Warwick, P.E. (2012), Lead pre-concentration using a novel manganese dioxide resin. *Environmental Earth Sciences*, **67** (3), 637-640.
101. Silva, M.M.F., Oliveira, M.M., Avelino, M.C., Fonseca, M.G., Almeida, R.K.S. and Silva, E.C. (2012), Adsorption of an industrial anionic dye by modified-KSF-montmorillonite: Evaluation of the kinetic, thermodynamic and equilibrium data. *Chemical Engineering Journal*, **203**), 259-268.
102. Hayati, B. and Mahmoodi, N.M. (2012), Modification of activated carbon by the alkaline treatment to remove the dyes from wastewater: mechanism, isotherm and kinetic. *Desalination and Water Treatment*, **47** (1-3), 322-333.
103. Sheng, G.D., Li, Y.M., Dong, H.P. and Shao, D.D. (2012), Environmental condition effects on radionuclide Cu-64(II) sequestration to a novel composite: polyaniline grafted multiwalled carbon nanotubes. *Journal of Radioanalytical and Nuclear Chemistry*, **293** (3), 797-806.
104. Adegoke, H.I. and Adekola, F.A. (2012), Equilibrium sorption of hexavalent chromium from aqueous solution using synthetic hematite. *Colloid Journal*, **74** (4), 420-426.
105. Wan, D.J., Liu, H.J., Liu, R.P., Qu, J.H., Li, S.S. and Zhang, J. (2012), Adsorption of nitrate and nitrite from aqueous solution onto calcined (Mg-Al) hydrotalcite of different Mg/Al ratio. *Chemical Engineering Journal*, **195**), 241-247.
106. Foo, K.Y. and Hameed, B.H. (2012), Preparation of activated carbon by microwave heating of langsat (Lansium domesticum) empty fruit bunch waste. *Bioresource Technology*, **116**), 522-525.
107. Mahmoodi, N.M. and Najafi, F. (2012), Preparation of surface modified zinc oxide nanoparticle with high capacity dye removal ability. *Materials Research Bulletin*, **47** (7), 1800-1809.
108. Manoochehri, M., Khorsand, A. and Hashemi, E. (2012), Role of Activated Carbon Modified by H3PO4 and K2CO3 From Natural Adsorbent for Removal of Pb (II) From Aqueous Solutions. *Carbon Letters*, **13** (3), 167-172.
109. Mahmoodi, N.M. and Najafi, F. (2012), Synthesis, amine functionalization and dye removal ability of titania/silica nano-hybrid. *Microporous and Mesoporous Materials*, **156**), 153-160.
110. Dittert, I.M., Vilar, V.J.P., da Silva, E.A.B., de Souza, S.M.A.G., de Souza, A.A.U., Botelho, C.M.S. and Boaventura, R.A.R. (2012), Adding value to marine macro-algae Laminaria digitata through its use in the separation and recovery of trivalent chromium ions from aqueous solution. *Chemical Engineering Journal*, **193**), 348-357.
111. Huang, J.H., Jin, X.Y., Mao, J.L., Yuan, B., Deng, R.J. and Deng, S.G. (2012), Synthesis, characterization and adsorption properties of diethylenetriamine-modified hypercrosslinked resins for efficient removal of salicylic acid from aqueous solution. *Journal of Hazardous Materials*, **217**), 406-415.
112. Foo, K.Y. and Hameed, B.H. (2012), Mesoporous activated carbon from wood sawdust by K2CO3 activation using microwave heating. *Bioresource Technology*, **111**), 425-432.
113. Foo, K.Y. and Hameed, B.H. (2012), Textural porosity, surface chemistry and adsorptive properties of durian shell derived activated carbon prepared by microwave assisted NaOH activation. *Chemical Engineering Journal*, **187**), 53-62.
114. Sousa, J., Freitas, O.M. and Figueiredo, S.A. (2012), Basic Dyestuffs Removal from Textile Effluents Using Feathers: Equilibrium, Kinetic and Column Studies. *Global Nest Journal*, **14** (1), 100-107.
115. Foo, K.Y. and Hameed, B.H. (2012), Coconut husk derived activated carbon via microwave induced activation: Effects of activation agents, preparation parameters and adsorption performance. *Chemical Engineering Journal*, **184**), 57-65.
116. Sekomo, C.B., Rousseau, D.P.L. and Lens, P.N.L. (2012), Use of Gisenyi Volcanic Rock for Adsorptive Removal of Cd(II), Cu(II), Pb(II), and Zn(II) from Wastewater. *Water Air and Soil Pollution*, **223** (2), 533-547.
117. Foo, K.Y. and Hameed, B.H. (2012), Factors affecting the carbon yield and adsorption capability of the mangosteen peel activated carbon prepared by microwave assisted K2CO3 activation. *Chemical Engineering Journal*, **180**), 66-74.
118. Sheng, G.D., Li, Y.M., Yang, X., Ren, X.M., Yang, S.T., Hu, J. and Wang, X.K. (2012), Efficient removal of arsenate by versatile magnetic graphene oxide composites. *Rsc Advances*, **2** (32), 12400-12407.
119. Minami, S., Miyoshi, T., Murayama, N. and Shibata, J. (2012), Adsorption of As by gamma-Fe2O3 and the Effect of Temperature. *Kagaku Kogaku Ronbunshu*, **38** (5), 318-323.
120. Khani, M.H. (2012), Biosorption of Strontium by a Nonliving Brown Marine Algae, Padina Sp. *Separation Science and Technology* , **47** (13), 1886-1897.
121. Safa, M., Larouci, M., Meddah, B. and Valemens, P. (2012), The sorption of lead, cadmium, copper and zinc ions from aqueous solutions on a raw diatomite from Algeria. *Water Science and Technology*, **65** (10), 1729-1737.
122. Guo, L., Liu, C.P., Guo, Z.L., Sun, L. and Liu, J.S. (2012), Preparation of Polyvinyl Chloride-Based Thiosemicarbazide Resin and Its Selective Adsorption of Ag(I) and Au(III). *Journal of Dispersion Science and Technology*, **33** (5), 690-696.
123. Guo, L., Li, G.Y., Liu, J.S., Meng, Y.F. and Xing, G.X. (2012), Nonlinear Analysis of the Kinetics and Equilibrium for Adsorptive Removal of Cd(II) by Starch Phosphate. *Journal of Dispersion Science and Technology*, **33** (1-3), 403-409.
124. Tang, R., Li, Q., Ding, L., Cui, H. and Zhai, J.P. (2012), Reactive sorption of mercury(II) on to poly(m-phenylenediamine) microparticles. *Environmental Technology*, **33** (3), 341-348.
125. Foo, K.Y. and Hameed, B.H. (2012), Preparation, characterization and evaluation of adsorptive properties of orange peel based activated carbon via microwave induced K2CO3 activation. *Bioresource Technology*, **104**), 679-686.
126. Ho, Y.S. (2012), Comment on “Biosorption of Cr(VI) from aqueous solutions onto Hydrilla verticillata weed: equilibrium, kinetics and thermodynamic studies”. *Environmental Engineering and Management Journal*, **11** (1), 231-232.
127. Foo, K.Y. and Hameed, B.H. (2012), Microwave-assisted preparation and adsorption performance of activated carbon from biodiesel industry solid reside: Influence of operational parameters. *Bioresource Technology*, **103** (1), 398-404.
128. Mahmoodi, N.M., Hayati, B. and Arami, M. (2012), Kinetic, equilibrium and thermodynamic studies of ternary system dye removal using a biopolymer. *Industrial Crops and Products*, **35** (1), 295-301.
129. Mahmoodi, N.M., Najafi, F., Khorramfar, S., Amini, F. and Arami, M. (2011), Synthesis, characterization and dye removal ability of high capacity polymeric adsorbent: Polyaminoimide homopolymer. *Journal of Hazardous Materials*, **198**), 87-94.
130. Ai, L.H., Zhang, C.Y., Liao, F., Wang, Y., Li, M., Meng, L.Y. and Jiang, J. (2011), Removal of methylene blue from aqueous solution with magnetite loaded multi-wall carbon nanotube: Kinetic, isotherm and mechanism analysis. *Journal of Hazardous Materials*, **198**), 282-290.
131. Yuh-Shan, H. (2011), Comments on “Recognition of molecularly imprinted polymers for a quaternary alkaloid of berberine”. *Talanta*, **87**), 311.
132. Tobbi, O., Guerfi, K. and Rebbani, N. (2011), Immobilization of Pb(II), Cd(II) Ions on Algerian Montmorillonite Surfaces from Aqueous Medium. *Sensor Letters*, **9** (6), 2404-2407.
133. Tang, R., Li, Q., Cui, H., Zhang, Y. and Zhai, J.P. (2011), Adsorption of aqueous Hg (II) by a novel poly(aniline-co-o-aminophenol)/mesoporous silica SBA-15 composite. *Polymers for Advanced Technologies*, **22** (12), 2231-2236.
134. Mahmoodi, N.M., Hayati, B., Bahrami, H. and Arami, M. (2011), Dye Adsorption and Desorption Properties of Mentha pulegium in Single and Binary Systems. *Journal of Applied Polymer Science*, **122** (3), 1489-1499.
135. Khani, M.H. (2011), Uranium biosorption by Padina sp algae biomass: kinetics and thermodynamics. *Environmental Science and Pollution Research*, **18** (9), 1593-1605.
136. Benavente, M., Moreno, L. and Martinez, J. (2011), Sorption of heavy metals from gold mining wastewater using chitosan. *Journal of the Taiwan Institute of Chemical Engineers*, **42** (6), 976-988.
137. Kayranli, B. (2011), Adsorption of textile dyes onto iron based waterworks sludge from aqueous solution; isotherm, kinetic and thermodynamic study. *Chemical Engineering Journal*, **173** (3), 782-791.
138. Foo, K.Y. and Hameed, B.H. (2011), Preparation and characterization of activated carbon from sunflower seed oil residue via microwave assisted K2CO3 activation. *Bioresource Technology*, **102** (20), 9794-9799.
139. Mahmoodi, N.M., Khorramfar, S. and Najafi, F. (2011), Amine-functionalized silica nanoparticle: Preparation, characterization and anionic dye removal ability. *Desalination*, **279** (1-3), 61-68.
140. Zhao, D.L., Zhang, C.C., Xu, J.Z. and Niu, Z.W. (2011), Impact of environmental conditions on sorption of Pb-210(II) to NKF-5 zeolite. *Journal of Radioanalytical and Nuclear Chemistry*, **289** (3), 671-678.
141. Li, J.X., Guo, Z.Q., Zhang, S.W. and Wang, X.K. (2011), Enrich and seal radionuclides in magnetic agarose microspheres. *Chemical Engineering Journal*, **172** (2-3), 892-897.
142. Tang, W.S., Li, Q., Gao, S.A. and Shang, J.K. (2011), Arsenic (III,V) removal from aqueous solution by ultrafine alpha-Fe2O3 nanoparticles synthesized from solvent thermal method. *Journal of Hazardous Materials*, **192** (1), 131-138.
143. Chen, L.H., Ramadan, A., Lu, L.L., Shao, W.J., Luo, F. and Chen, J. (2011), Biosorption of Methylene Blue from Aqueous Solution Using Lawny Grass Modified with Citric Acid. *Journal of Chemical and Engineering Data*, **56** (8), 3392-3399.
144. Ai, L.H., Li, M. and Li, L. (2011), Adsorption of Methylene Blue from Aqueous Solution with Activated Carbon/Cobalt Ferrite/Alginate Composite Beads: Kinetics, Isotherms, and Thermodynamics. *Journal of Chemical and Engineering Data*, **56** (8), 3475-3483.
145. Mahmoodi, N.M., Hayati, B., Arami, M. and Bahrami, H. (2011), Preparation, characterization and dye adsorption properties of biocompatible composite (alginate/titania nanoparticle). *Desalination*, **275** (1-3), 93-101.
146. Zhao, D.L., Sheng, G.D., Hu, J., Chen, C.L. and Wang, X.K. (2011), The adsorption of Pb(II) on Mg2Al layered double hydroxide. *Chemical Engineering Journal*, **171** (1), 167-174.
147. Mahmoodi, N.M. (2011), Equilibrium, Kinetics, and Thermodynamics of Dye Removal Using Alginate in Binary Systems. *Journal of Chemical and Engineering Data*, **56** (6), 2802-2811.
148. Katsou, E., Malamis, S., Tzanoudaki, M., Haralambous, K.J. and Loizidou, M. (2011), Regeneration of natural zeolite polluted by lead and zinc in wastewater treatment systems. *Journal of Hazardous Materials*, **189** (3), 773-786.
149. Mahmoodi, N.M., Salehi, R. and Arami, M. (2011), Binary system dye removal from colored textile wastewater using activated carbon: Kinetic and isotherm studies. *Desalination*, **272** (1-3), 187-195.
150. Guo, L., Li, G.Y., Liu, J.S., Ma, S.M. and Zhang, J.F. (2011), Kinetic and Equilibrium Studies on Adsorptive Removal of Toluidine Blue by Water-Insoluble Starch Sulfate. *Journal of Chemical and Engineering Data*, **56** (5), 1875-1881.
151. Katsou, E., Malamis, S. and Haralambous, K. (2011), Pre-treatment of Industrial Wastewater Polluted with Lead Using Adsorbents and Ultrafiltration or Microfiltration Membranes. *Water Environment Research*, **83** (4), 298-312.
152. Ho, Y.S. (2011), Comment on “Adsorption mechanism of selenate and selenite on the binary oxide systems” by Y.T. Chan et al. [Water Research 43 (2009) 4412-4420]. *Water Research*, **45** (7), 2437.
153. Ofomaja, A.E. (2011), Kinetics and pseudo-isotherm studies of 4-nitrophenol adsorption onto mansonia wood sawdust. *Industrial Crops and Products*, **33** (2), 418-428.
154. Tseng, R.L., Wu, P.H., Wu, F.C. and Juang, R.S. (2011), Half-life and half-capacity concentration approach for the adsorption of 2,4-dichlorophenol and methyl blue from water on activated carbons. *Journal of the Taiwan Institute of Chemical Engineers*, **42** (2), 312-319.
155. Mahmoodi, N.M., Hayati, B., Arami, M. and Lan, C. (2011), Adsorption of textile dyes on Pine Cone from colored wastewater: Kinetic, equilibrium and thermodynamic studies. *Desalination*, **268** (1-3), 117-125.
156. Mahmoodi, N.M., Salehi, R., Arami, M. and Bahrami, H. (2011), Dye removal from colored textile wastewater using chitosan in binary systems. *Desalination*, **267** (1), 64-72.
157. Hu, J., Shao, D.D., Chen, C.L., Sheng, G.D., Ren, X.M. and Wang, X.K. (2011), Removal of 1-naphthylamine from aqueous solution by multiwall carbon nanotubes/iron oxides/cyclodextrin composite. *Journal of Hazardous Materials*, **185** (1), 463-471.
158. Rajeshkannan, R., Rajasimman, M. and Rajamohan, N. (2011), Decolourization of Malachite Green Using Tamarind Seed: Optimization, Isotherm and Kinetic Studies. *Chemical Industry & Chemical Engineering Quarterly*, **17** (1), 67-79.
159. Rajeshkannan, R., Rajasimman, M. and Rajamohan, N. (2011), Sorption of Acid Blue 9 Using Hydrilla verticillata BiomassOptimization, Equilibrium, and Kinetics Studies. *Bioremediation Journal*, **15** (1), 57-67.
160. Lin, J.X. and Wang, L. (2011), Treatment of textile wastewater using organically modified bentonite. *Desalination and Water Treatment*, **25** (1-3), 25-30.
161. Sonar, N.L., Pardeshi, V., De, V., Shukla, R., Valsala, T.P., Sonavane, M.S., Kulkarni, Y., Manoj, N., Pillai, C.S., Tyagi, A.K., Raj, K. and Manchanda, V.K. (2011), Evaluation of Metal Antimonate Compounds for the Removal of Radiostrontium from Radioactive Liquid Waste: Characterization and Sorption Behavior. *Separation Science and Technology*, **46** (11), 1776-1787.
162. AL-Ghezawi, N., Al-Anber, M.A., Al-Anber, Z.A., El-Hasan, T. and Al-Momani, I. (2010), Decontamination and adsorption modelling of aqueous Pb2+ and Co2+ ions using natural inorganic materials: tripoli (NT) and bentonite (NB). *Desalination and Water Treatment*, **24** (1-3), 336-343.
163. Mahmoodi, N.M., Hayati, B. and Arami, M. (2010), Textile Dye Removal from Single and Ternary Systems Using Date Stones: Kinetic, Isotherm, and Thermodynamic Studies. *Journal of Chemical and Engineering Data*, **55** (11), 4638-4649.
164. Mahmoodi, N.M., Hayati, B., Arami, M. and Mazaheri, F. (2010), Single and Binary System Dye Removal from Colored Textile Wastewater by a Dendrimer as a Polymeric Nanoarchitecture: Equilibrium and Kinetics. *Journal of Chemical and Engineering Data*, **55** (11), 4660-4668.
165. Ru-Ling, T., Wu, K.T., Wu, F.C. and Juang, R.S. (2010), Kinetic studies on the adsorption of phenol, 4-chlorophenol, and 2,4-dichlorophenol from water using activated carbons. *Journal of Environmental Management*, **91** (11), 2208-2214.
166. Salehi, R., Arami, M., Mahmoodi, N.M., Bahrami, H. and Khorramfar, S. (2010), Novel biocompatible composite (Chitosan-zinc oxide nanoparticle): Preparation, characterization and dye adsorption properties. *Colloids and Surfaces B-Biointerfaces*, **80** (1), 86-93.
167. Ho, Y.S. (2010), Comment on “Acid Green 25 removal from wastewater by organo-bentonite from Pacitan” by R. Koswojo, R. P. Utomo, Y.-H. Ju, A. Ayucitra, F. E. Soetaredjo, J. Sunarso, S. Ismadji [Applied Clay Science 48 (2010) 81-86]. *Applied Clay Science*, **50** (1), 164.
168. Utomo, R.P., Koswojo, R., Ju, Y.H., Ayucitra, A., Soetaredjo, F.E., Sunarso, J. and Ismadji, S. (2010), Reply to the comment on “Acid Green 25 removal from wastewater by organo-bentonite from Pacitan” by R. Koswojo, R. P. Utomo, Y.-H. Ju, A. Ayucitra, F. E. Soetaredjo, J. Sunarso, S. Ismadji [Applied Clay Science 48 (2010) 81-86]. *Applied Clay Science*, **50** (1), 165-166.
169. Rajeshkannan, R., Rajasimman, M. and Rajamohan, N. (2010), Optimization, equilibrium and kinetics studies on sorption of Acid Blue 9 using brown marine algae Turbinaria conoides. *Biodegradation*, **21** (5), 713-727.
170. Kannan, R.R., Rajasimman, M., Rajamohan, N. and Sivaprakash, B. (2010), Equilibrium and Kinetic Studies on Sorption of Malachite Green using Hydrilla Verticillata Biomass. *International Journal of Environmental Research*, **4** (4), 817-824.
171. Ali, I.M., Zakaria, E.S. and Aly, H.F. (2010), Highly effective removal of Na-22, Cs-134 and Co-60 from aqueous solutions by titanosilicate: a radiotracer study. *Journal of Radioanalytical and Nuclear Chemistry*, **285** (3), 483-489.
172. Rao, K.S., Anand, S. and Venkateswarlu, P. (2010), Cadmium removal from aqueous solutions using biosorbent Syzygium cumini leaf powder: Kinetic and equilibrium studies. *Korean Journal of Chemical Engineering*, **27** (5), 1547-1554.
173. Malash, G.F. and El-Khaiary, M.I. (2010), Methylene blue adsorption by the waste of Abu-Tartour phosphate rock. *Journal of Colloid and Interface Science*, **348** (2), 537-545.
174. Ho, Y.S. (2010), Comments on “Adsorption Performance of Nickel and Cadmium Ions Onto Brewer’S Yeast”. *Canadian Journal of Chemical Engineering*, **88** (4), 693-694.
175. Ho, Y.S. (2010), Comments on using of “pseudo-second-order rate equation” in Journal of Radioanalytical and Nuclear Chemistry, Volume 283. *Journal of Radioanalytical and Nuclear Chemistry*, **285** (2), 403.
176. Ren, X.M., Wang, S.W., Yang, S.T. and Li, J.X. (2010), Response to the comments of Y. S. Ho to the paper “Influence of contact time, pH, soil humic/fulvic acids, ionic strength and temperature on sorption of U(VI) onto MX-80 bentonite” by Ren XM, Wang SW, Yang ST, and Li JX published in J. Radioanal. Nucl. Chem. 283 (2010) 253. *Journal of Radioanalytical and Nuclear Chemistry*, **285** (2), 405.
177. Ho, Y.S. (2010), Comments on “Preparation and application of 4-amino-4’-nitro azobenzene modified chitosan as a selective adsorbent for the determination of Au(III) and Pd(II)”. *Microchimica Acta*, **170** (1-2), 187.
178. Wang, H.F., Bao, C.L., Li, F., Kong, X.F. and Xu, J.J. (2010), Reply to the Comments on “Preparation and application of 4-amino-4’-nitroazobenzene modified chitosan as a selective adsorbent for the determination of Au(III) and Pd(II)”. *Microchimica Acta*, **170** (1-2), 189.
179. Ho, Y.S. (2010), Comments on using of “initial adsorption rate” [J. Hazard. Mater. 173]. *Journal of Hazardous Materials*, **179** (1-3), 1165.
180. El-Khaiary, M.I., Malash, G.F. and Ho, Y.S. (2010), On the use of linearized pseudo-second-order kinetic equations for modeling adsorption systems. *Desalination*, **257** (1-3), 93-101.
181. Oliveira, F.D., Soares, A.C., Freitas, O.M. and Figueiredo, S.A. (2010), Copper, Nickel and Zinc Removal by Peanut Hulls: Batch and Column Studies in Mono, Tri-Component Systems and with Real Effluent. *Global Nest Journal*, **12** (2), 206-214.
182. Li, K.Q., Li, Y. and Zheng, Z. (2010), Kinetics and mechanism studies of p-nitroaniline adsorption on activated carbon fibers prepared from cotton stalk by NH4H2PO4 activation and subsequent gasification with steam.  *Journal of Hazardous Materials*, **178** (1-3), 553-559.
183. Ho, Y.S. (2010), Comments on “Removal and recovery of Cu(II) and Zn(II) using immobilized Mentha arvensis distillation waste biomass”. *Ecological Engineering*, **36** (6), 832.
184. Hu, J., Xie, Z., He, B., Sheng, G.D., Chen, C.L., Li, J.X., Chen, Y.X. and Wang, X.K. (2010), Sorption of Eu(III) on GMZ bentonite in the absence/presence of humic acid studied by batch and XAFS techniques. *Science China-Chemistry*, **53** (6), 1420-1428.
185. Ofomaja, A.E., Naidoo, E.B. and Modise, S.J. (2010), Kinetic and Pseudo-Second-Order Modeling of Lead Biosorption onto Pine Cone Powder. *Industrial & Engineering Chemistry Research*, **49** (6), 2562-2572.
186. Tsai, W.T. and Chen, H.R. (2010), Removal of malachite green from aqueous solution using low-cost chlorella-based biomass. *Journal of Hazardous Materials*, **175** (1-3), 844-849.
187. Kannan, R.R., Rajasimman, M., Rajamohan, N. and Sivaprakash, B. (2010), Brown marine algae turbinaria conoides as biosorbent for Malachite green removal: Equilibrium and kinetic modeling. *Frontiers of Environmental Science & Engineering in China*, **4** (1), 116-122.
188. Ofomaja, A.E., Naidoo, E.B. and Modise, S.J. (2010), Dynamic studies and pseudo-second order modeling of copper(II) biosorption onto pine cone powder. *Desalination*, **251** (1-3), 112-122.
189. Al-Anber, M.A. (2010), Removal of high-level Fe(3+) from aqueous solution using natural inorganic materials: Bentonite (NB) and quartz (NQ). *Desalination*, **250** (3), 885-891.
190. Rao, K.S., Anand, S. and Venkateswarlu, P. (2010), Psidium guvajava L Leaf Powder - A Potential Low-cost Biosorbent for the Removal of Cadmium(II) Ions from Wastewater. *Adsorption Science & Technology*, **28** (2), 163-178.
191. Zamora, F., Sabio, E., Roman, S., Gonzalez-Garcia, C.M. and Ledesma, B. (2010), Modelling the Adsorption of p-Nitrophenol by the Boyd Method in Conjunction with the Finite Element Method. *Adsorption Science & Technology*, **28** (8-9), 671-687.
192. Rao, K.S., Anand, S. and Venkateswarlu, P. (2010), Adsorption of Cadmium(Ii) Ions from Aqueous Solution by Tectona Grandis Lf (Teak Leaves Powder). *Bioresources*, **5** (1), 438-U26.
193. He, X.J., Yao, L., Liang, Z. and Ni, J.R. (2010), Paper sludge as a feasible soil amendment for the immobilization of Pb2+. *Journal of Environmental Sciences-China*, **22** (3), 413-420.
194. Ali, I.M. (2009), Sorption studies of Cs-134, Co-60 and Eu152+154 on phosphoric acid activated silico-antimonate crystals in high acidic media. *Chemical Engineering Journal*, **155** (3), 580-585.
195. Singh, K.P., Ojha, P., Malik, A. and Jain, G. (2009), Partial least squares and artificial neural networks modeling for predicting chlorophenol removal from aqueous solution. *Chemometrics and Intelligent Laboratory Systems*, **99** (2), 150-160.
196. Ho, Y.S. (2009), Comments on “Defluoridation of water using neodymium-modified chitosan” Discussion. *Journal of Hazardous Materials*, **172** (1), 515.
197. Lin, J.X. and Wang, L. (2009), Comment on “Adsorption of Supranol Yellow 4 GL from aqueous solution by surfactant-treated aluminum/chromium-intercalated bentonite” Discussion. *Journal of Hazardous Materials*, **172** (1), 516-517.
198. Guo, L., Li, G.Y., Liu, J.S., Yin, P. and Li, Q. (2009), Adsorption of Aniline on Cross-Linked Starch Sulfate from Aqueous Solution. *Industrial & Engineering Chemistry Research*, **48** (23), 10657-10663.
199. Plazinski, W., Rudzinski, W. and Plazinska, A. (2009), Theoretical models of sorption kinetics including a surface reaction mechanism: A review. *Advances in Colloid and Interface Science*,  **152** (1-2), 2-13.
200. Wajima, T., Umeta, Y., Narita, S. and Sugawara, K. (2009), Adsorption behavior of fluoride ions using a titanium hydroxide-derived adsorbent. *Desalination*, **249** (1), 323-330.
201. Huang, J.H. (2009), Adsorption properties of a microporous and mesoporous hyper-crosslinked polymeric adsorbent functionalized with phenoxy groups for phenol in aqueous solution. *Journal of Colloid and Interface Science*, **339** (2), 296-301.
202. Ho, Y.S. (2009), Comments on “Kinetics of naphthalene adsorption on an activated carbon: Comparison between aqueous and organic media” by B. Cabal et al. [Chemosphere 76 (4) (2009) 433-438]. *Chemosphere*, **77** (10), 1453.
203. Ania, C.O. (2009), Reply to Comments by Yuh-Shan Ho on “Kinetics of naphthalene adsorption on an activated carbon: Comparison between aqueous and organic media” [Chemosphere 76 (4) (2009) 433-438]. *Chemosphere*, **77** (10), 1454.
204. Cheng, X., Huang, X.R., Wang, X.Z., Zhao, B.Q., Chen, A.Y. and Sun, D.Z. (2009), Phosphate adsorption from sewage sludge filtrate using zinc-aluminum layered double hydroxides. *Journal of Hazardous Materials*, **169** (1-3), 958-964.
205. Lin, J.X. and Wang, L. (2009), Comparison between linear and non-linear forms of pseudo-first-order and pseudo-second-order adsorption kinetic models for the removal of methylene blue by activated carbon. *Frontiers of Environmental Science & Engineering in China*, **3** (3), 320-324.
206. Boutemedjet, S. and Hamdaoui, O. (2009), Sorption of malachite green by eucalyptus bark as a non-conventional low-cost biosorbent. *Desalination and Water Treatment*, **8** (1-3), 201-210.
207. Tsai, W.T., Hsien, K.J. and Hsu, H.C. (2009), Adsorption of organic compounds from aqueous solution onto the synthesized zeolite. *Journal of Hazardous Materials*, **166** (2-3), 635-641.
208. Li, K.Q., Zheng, Z., Feng, J.W., Zhang, J.B., Luo, X.Z., Zhao, G.H. and Huang, X.F. (2009), Adsorption of p-nitroaniline from aqueous solutions onto activated carbon fiber prepared from cotton stalk. *Journal of Hazardous Materials*, **166** (2-3), 1180-1185.
209. Li, K.Q., Zheng, Z., Huang, X.F., Zhao, G.H., Feng, J.W. and Zhang, J.B. (2009), Equilibrium, kinetic and thermodynamic studies on the adsorption of 2-nitroaniline onto activated carbon prepared from cotton stalk fibre. *Journal of Hazardous Materials*, **166** (1), 213-220.
210. Ho, Y.S. (2009), Comments on “Adsorption of Ga(III) on Oxidized Coir”. *Industrial & Engineering Chemistry Research*, **48** (12), 5920.
211. Li, K.L. and Wang, X.H. (2009), Adsorptive removal of Pb(II) by activated carbon prepared from Spartina alterniflora: Equilibrium, kinetics and thermodynamics. *Bioresource Technology*, **100** (11), 2810-2815.
212. Ozmetin, C., Aydin, O., Kocakerim, M.M., Korkmaz, M. and Ozmetin, E. (2009), An empirical kinetic model for calcium removal from calcium impurity-containing saturated boric acid solution by ion exchange technology using Amberlite IR-120 resin. *Chemical Engineering Journal*, **148** (2-3), 420-424.
213. Kumar, K.V. and Porkodi, K. (2009), Modelling the solid-liquid adsorption processes using artificial neural networks trained by pseudo second order kinetics. *Chemical Engineering Journal*, **148** (1), 20-25.
214. Wu, C.H. (2009), Response to comment on “Adsorption of direct dyes from aqueous solutions by carbon nanotubes: Determination of equilibrium, kinetics and thermodynamics parameter” by Dr. Ho. *Journal of Colloid and Interface Science*, **333** (1), 413-414.
215. Wan, D.J., Liu, H.J., Zhao, X., Qu, J.H., Xiao, S.H. and Hou, Y.N. (2009), Role of the Mg/Al atomic ratio in hydrotalcite-supported Pd/Sn catalysts for nitrate adsorption and hydrogenation reduction. *Journal of Colloid and Interface Science*, **332** (1), 151-157.
216. Hu, J., Chen, C.L., Zhu, X.X. and Wang, X.K. (2009), Removal of chromium from aqueous solution by using oxidized multiwalled carbon nanotubes. *Journal of Hazardous Materials*, **162** (2-3), 1542-1550.
217. Khambhaty, Y., Mody, K., Basha, S. and Jha, B. (2009), Biosorption of Inorganic Mercury onto Dead Biomass of Marine Aspergillus niger: Kinetic, Equilibrium, and Thermodynamic Studies. *Environmental Engineering Science*, **26** (3), 531-539.
218. Ilic, V., Radojevic, D., Mihailovic, D., Radetic, M. and Jovancic, P. (2009), The Study of Sorption of Toxic Basic Dyes from Aqueous Solutions on H2O2 Treated Recycled Wool-based Nonwoven Material and Related Toxicity Analysis. *Textile Research Journal*, **79** (3), 253-260.
219. Zafar, M.N., Abbas, I., Nadeem, R., Sheikh, M.A. and Ghauri, M.A. (2009), Removal of Nickel onto Alkali Treated Rice Bran. *Water Air and Soil Pollution*, **197** (1-4), 361-370.
220. Benguella, B. and Yacouta-Nour, A. (2009), Adsorption of Bezanyl Red and Nylomine Green from aqueous solutions by natural and acid-activated bentonite. *Desalination*, **235** (1-3), 276-292.
221. Guo, L., Sun, C.M., Li, G.Y., Liu, C.P. and Ji, C.N. (2009), Thermodynamics and kinetics of Zn(II) adsorption on crosslinked starch phosphates. *Journal of Hazardous Materials*, **161** (1), 510-515.
222. Ghodbane, I. and Hamdaoui, O. (2008), Removal of mercury(II) from aqueous media using eucalyptus bark: Kinetic and equilibrium studies.  *Journal of Hazardous Materials*, **160** (2-3), 301-309.
223. Hameed, B.H. and El-Khaiary, M.I. (2008), Malachite green adsorption by rattan sawdust: Isotherm, kinetic and mechanism modeling. *Journal of Hazardous Materials*, **159** (2-3), 574-579.
224. Apiratikul, R. and Pavasant, P. (2008), Sorption of Cu2+, Cd2+, and Pb2+ using modified zeolite from coal fly ash. *Chemical Engineering Journal*, **144** (2), 245-258.
225. Khambhaty, Y., Mody, K., Basha, S. and Jha, B. (2008), Pseudo-second-order kinetic models for the sorption of Hg(II) onto dead biomass of marine Aspergillus niger: Comparison of linear and non-linear methods. *Colloids and Surfaces A-Physicochemical and Engineering Aspects*, **328** (1-3), 40-43.
226. Hamdaoui, O., Saoudi, F., Chiha, M. and Naffrechoux, E. (2008), Sorption of malachite green by a novel sorbent, dead leaves of plane tree: Equilibrium and kinetic modeling. *Chemical Engineering Journal*, **143** (1-3), 73-84.
227. Mahmoodi, N.M. and Arami, M. (2008), Modeling and sensitivity analysis of dyes adsorption onto natural adsorbent from colored textile wastewater. *Journal of Applied Polymer Science*, **109** (6), 4043-4048.
228. Hameed, B.H. and El-Khaiary, M.I. (2008), Equilibrium, kinetics and mechanism of malachite green adsorption on activated carbon prepared from bamboo by K2CO3 activation and subsequent gasification with CO2. *Journal of Hazardous Materials*, **157** (2-3), 344-351.
229. Arshad, M., Zafar, M.N., Younis, S. and Nadeem, R. (2008), The use of Neem biomass for the biosorption of zinc from aqueous solutions. *Journal of Hazardous Materials*, **157** (2-3), 534-540.
230. Lin, J.X., Zhan, S.L., Fang, M.H. and Yang, H. (2008), Comment on “Experimental study and modeling of basic dye sorption by diatomaceous clay”. *Applied Clay Science*, **41** (1-2), 105-106.
231. Ho, Y.S. (2008), Sol-gel-immobilized recombinant E-coli for biosorption of Cd(2+). *Journal of the Chinese Institute of Chemical Engineers*, **39** (5), 539.
232. Bannari, A., Proulx, P., Menard, H. and Cirtiu, C.M. (2008), Mathematical modeling of the kinetics of phenol electrocatalytic hydrogenation over supported Pd-alumina catalyst. *Applied Catalysis A-General*, **345** (1), 28-42.
233. Oladoja, N.A., Aboluwoye, C.O., Oladimeji, Y.B., Ashogbon, A.O. and Otemuyiwa, I.O. (2008), Studies on castor seed shell as a sorbent in basic dye contaminated wastewater remediation. *Desalination*, **227** (1-3), 190-203.
234. Hameed, B.H. and El-Khaiary, M.I. (2008), Removal of basic dye from aqueous medium using a novel agricultural waste material: Pumpkin seed hull. *Journal of Hazardous Materials*, **155** (3), 601-609.
235. Hameed, B.H. and El-Khaiary, M.I. (2008), Batch removal of malachite green from aqueous solutions by adsorption on oil palm trunk fibre: Equilibrium isotherms and kinetic studies. *Journal of Hazardous Materials*, **154** (1-3), 237-244.
236. Hameed, B.H. and El-Khaiary, M.I. (2008), Sorption kinetics and isotherm studies of a cationic dye using agricultural waste: Broad bean peels. *Journal of Hazardous Materials*, **154** (1-3), 639-648.
237. Ho, Y.S. (2008), Comments on “Adsorption behavior of heavy metal ions by carbon nanotubes grown on microsized Al2O3 particles”. *Journal of University of Science and Technology Beijing*, **15** (3), 366.
238. Abbas, M., Nadeem, R., Zafar, M.N. and Arshad, M. (2008), Biosorption of chromium (III) and chromium (VI) by untreated and pretreated Cassia fistula biomass from aqueous solutions. *Water Air and Soil Pollution*, **191** (1-4), 139-148.
239. Arami, M., Limaee, N.Y. and Mahmoodi, N.M. (2008), Evaluation of the adsorption kinetics and equilibrium for the potential removal of acid dyes using a biosorbent. *Chemical Engineering Journal*, **139** (1), 2-10.
240. Apiratikul, R. and Pavasant, P. (2008), Batch and column studies of biosorption of heavy metals by Caulerpa lentillifera. *Bioresource Technology*, **99** (8), 2766-2777.
241. Sener, S. (2008), Use of solid wastes of the soda ash plant as an adsorbent for the removal of anionic dyes: Equilibrium and kinetic studies. *Chemical Engineering Journal*, **138** (1-3), 207-214.
242. Al-Anber, M. and Al-Anber, Z.A. (2008), Utilization of natural zeolite as ion-exchange and sorbent material in the removal of iron. *Desalination*, **225** (1-3), 70-81.
243. Djeribi, R. and Hamdaoui, O. (2008), Sorption of copper(II) from aqueous solutions by cedar sawdust and crushed brick. *Desalination*, **225** (1-3), 95-112.
244. Hameed, B.H. and El-Khaiary, M.I. (2008), Kinetics and equilibrium studies of malachite green adsorption on rice straw-derived char. *Journal of Hazardous Materials*, **153** (1-2), 701-708.
245. Lin, J.X., Zhan, S.L., Fang, M.H. and Qian, X.Q. (2008), Study on the adsorption of dyes using diatomite and activated carbon. *Rare Metal Materials and Engineering*, **37**), 682-685.
246. Lin, J.X., Zhan, S.L., Fang, M.H., Qian, X.Q. and Yang, H. (2008), Adsorption of basic dye from aqueous solution onto fly ash. *Journal of Environmental Management*, **87** (1), 193-200.
247. Ghodbane, I., Nouri, L., Hamdaoui, O. and Chiha, M. (2008), Kinetic and equilibrium study for the sorption of cadmium(II) ions from aqueous phase by eucalyptus bark. *Journal of Hazardous Materials*, **152** (1), 148-158.
248. Vilar, V.J.P., Botelho, C.M.S. and Boaventura, R.A.R. (2008), Copper removal by algae Gelidium, agar extraction algal waste and granulated algal waste: Kinetics and equilibrium. *Bioresource Technology*, **99** (4), 750-762.
249. Adebowale, K.O., Unuabonah, E.I. and Olu-Owolabi, B.I. (2008), Kinetic and thermodynamic aspects of the adsorption of Pb2+ and Cd2+ ions on tripolyphosphate-modified kaolinite clay. *Chemical Engineering Journal*, **136** (2-3), 99-107.
250. Hasan, M., Ahmad, A.L. and Hameed, B.H. (2008), Adsorption of reactive dye onto cross-linked chitosan/oil palm ash composite beads. *Chemical Engineering Journal*, **136** (2-3), 164-172.
251. Benaissa, H. (2008), Removal of acid dyes from aqueous solutions using orange peel as a sorbent material. *International Journal of Environment and Pollution*, **34** (1-4), 71-82.
252. Matis, K.A., Zouboulis, A.I., Lazaridis, N.K. and Karapantsios, T.D. (2008), Metal ions biosorption from dilute aqueous solution. *International Journal of Environment and Pollution*, **34** (1-4), 231-245.
253. Ofomaja, A.E. and Ho, Y.S. (2008), Kinetic biosorption study of cadmium onto coconut copra meal as biosorbent. *International Journal of Environment and Pollution*, **34** (1-4), 466-476.
254. Khambhaty, Y., Mody, K., Basha, S. and Jha, B. (2008), Hg(II) removal from aqueous solution by dead fungal biomass of marine Aspergillus niger: Kinetic studies. *Separation Science and Technology*, **43** (5), 1221-1238.
255. Lin, J.X., Zhan, S.L., Fang, M.H. and Qian, X.Q. (2007), The adsorption of dyes from aqueous solution using diatomite. *Journal of Porous Materials*, **14** (4), 449-455.
256. Jeong, Y., Fan, M., Singh, S., Chuang, C.L., Saha, B. and van Leeuwen, H. (2007), Evaluation of iron oxide and aluminum oxide as potential arsenic(V) adsorbents. *Chemical Engineering and Processing*, **46** (10), 1030-1039.
257. Nouri, L., Ghodbane, I., Hamdaoui, O. and Chiha, M. (2007), Batch sorption dynamics and equilibrium for the removal of cadmium ions from aqueous phase using wheat bran. *Journal of Hazardous Materials*, **149** (1), 115-125.
258. Fu, L., Huang, X.H. and Wang, H.Y. (2007), Removal of supranol Yellow 4GL by adsorption onto Cr-intercalated montmorillonite - Comment.  *Journal of Hazardous Materials*, **148** (3), 771-772.
259. Chen, Y.X., Liu, S.Y. and Wang, G.Y. (2007), A kinetic investigation of cationic starch adsorption and flocculation in kaolin suspension. *Chemical Engineering Journal*, **133** (1-3), 325-333.
260. Nouri, L. and Hamdaoui, O. (2007), Ultrasonication-assisted sorption of cadmium from aqueous phase by wheat bran. *Journal of Physical Chemistry A*, **111** (34), 8456-8463.
261. El-Khaiary, M.I. (2007), Kinetics and mechanism of adsorption of methylene blue from aqueous solution by nitric-acid treated water-hyacinth. *Journal of Hazardous Materials*, **147** (1-2), 28-36.
262. Kumar, K.V. and Porkodi, K. (2007), Comments on “Biosorption of nickel from protonated rice bran”. *Journal of Hazardous Materials*, **147** (1-2), 679.
263. Unuabonah, E.I., Adebowale, K.O. and Olu-Owolabi, B.I. (2007), Kinetic and thermodynamic studies of the adsorption of lead (II) ions onto phosphate-modified kaolinite clay. *Journal of Hazardous Materials*, **144** (1-2), 386-395.
264. Sagar, N.P. and Shigh, U.K. (2007), Sorption dynamics of phenol on naturally occuring low cost clay. *Research Journal of Chemistry and Environment*, **11** (2), 23-28.
265. Porkodi, K. and Kumar, K.V. (2007), Equilibrium, kinetics and mechanism modeling and simulation of basic and acid dyes sorption onto jute fiber carbon: Eosin yellow, malachite green and crystal violet single component systems. *Journal of Hazardous Materials*, **143** (1-2), 311-327.
266. Alvarez-Ayuso, E., Garcia-Sanchez, A. and Querol, X. (2007), Adsorption of Cr(VI) from synthetic solutions and electroplating wastewaters on amorphous aluminium oxide. *Journal of Hazardous Materials*, **142** (1-2), 191-198.
267. Nayak, P.S. and Singh, B.K. (2007), Sorption studies on clay for the removal of phenol and p-nitrophenol from aqueous solution. *Indian Journal of Chemistry Section A-Inorganic Bio-Inorganic Physical Theoretical & Analytical Chemistry*, **46** (4), 620-623.
268. Hamdaoui, O. and Chiha, M. (2007), Removal of methylene blue from aqueous solutions by wheat bran. *Acta Chimica Slovenica*, **54** (2), 407-418.
269. Ho, Y.S. (2007), Comments on “An adsorption and kinetic study of lac dyeing on silk”. *Dyes and Pigments*, **72** (1), 134-136.
270. Ozmetin, C. and Aydin, O. (2007), A semi-empirical model for adsorption of magnesium ion from magnesium impurity-containing saturated boric acid solutions on Amberlite IR-120 resin. *Fresenius Environmental Bulletin*, **16** (7), 720-725.
271. Alam, M.Z., Muyibi, S.A., Mansor, M.F. and Wahid, R. (2007), Activated carbons derived from oil palm empty-fruit bunches: Application to environmental problems. *Journal of Environmental Sciences*, **19** (1), 103-108.
272. Alam, M.Z., Muyibi, S.A. and Toramae, J. (2007), Statistical optimization of adsorption processes for removal of 2,4-dichlorophenol by activated carbon derived from oil palm empty fruit bunches. *Journal of Environmental Sciences-China*, **19** (6), 674-677.
273. Arami, M., Limaee, N.Y. and Mahmoodi, N.M. (2006), Investigation on the adsorption capability of egg shell membrane towards model textile dyes. *Chemosphere*, **65** (11), 1999-2008.
274. de Castro, F.H.B., Garcia, G.B., de Hoces, M.C., Lara, M.A.M. and Jimenez, A.M. (2006), Use of solid of olive tree remainders in the biosorption of chromium. *Afinidad*, **63** (526), 454-460.
275. Kumar, K.V. (2006), Linear and non-linear regression analysis for the sorption kinetics of methylene blue onto activated carbon. *Journal of Hazardous Materials*, **137** (3), 1538-1544.
276. Ho, Y.S. (2006), Review of second-order models for adsorption systems. *Journal of Hazardous Materials*, **136** (3), 681-689.
277. Kumar, K.V. (2006), A note on the comments by Dr. Y.S. Ho on “Remediation of soil contaminated with the heavy metal (Cd2+)”. *Journal of Hazardous Materials*, **136** (3), 993-994.
278. Kumar, K.V. (2006), A note on the comments by Dr. Y.S. Ho on “Nitrate removal from aqueous solution by adsorption onto various materials”. *Journal of Hazardous Materials*, **136** (3), 995-996.
279. Arami, M., Limaee, N.Y., Mahmoodi, N.M. and Tabrizi, N.S. (2006), Equilibrium and kinetics studies for the adsorption of direct and acid dyes from aqueous solution by soy meal hull. *Journal of Hazardous Materials*, **135** (1-3), 171-179.
280. Tsai, W.T., Hsu, H.C., Su, T.Y., Lin, K.Y. and Lin, C.M. (2006), Adsorption characteristics of bisphenol-A in aqueous solutions onto hydrophobic zeolite. *Journal of Colloid and Interface Science*, **299** (2), 513-519.
281. Ho, Y.S. (2006), Comment on “Remediation of soil contaminated with the heavy metal (Cd2+)”. *Journal of Hazardous Materials*, **134** (1-3), 41-42.
282. Benaissa, H. (2006), Screening of new sorbent materials for cadmium removal from aqueous solutions. *Journal of Hazardous Materials*, **132** (2-3), 189-195.
283. Ho, Y.S. (2006), Comment on equilibrium and kinetics studies of adsorption of copper(II) on chitosan and chitosan/PVA beads. *International Journal of Biological Macromolecules*, **38** (2), 148-149.
284. Yaneva, Z. and Koumanova, B. (2006), Comparative modelling of mono- and dinitrophenols sorption on yellow bentonite from aqueous solutions. *Journal of Colloid and Interface Science*, **293** (2), 303-311.
285. Peng, S.C., Wang, S.H., Chen, T.H., Jiang, S.T. and Huang, C.H. (2006), Adsorption kinetics of methylene blue from aqueous solutions onto palygorskite. *Acta Geologica Sinica-English Edition*, **80** (2), 236-242.
286. Alam, M.Z., Muyibi, S.A., Mansor, M.F. and Wahid, R. (2006), Removal of phenol by activated carbons prepared from palm oil mill effluent sludge. *Journal of Environmental Sciences-China*, **18** (3), 446-452.
287. Ho, Y.S. (2006), Second-order kinetic model for the sorption of cadmium onto tree fern: A comparison of linear and non-linear methods. *Water Research*, **40** (1), 119-125.
288. Mane, S.M., Vanjara, A.K. and Sawant, M.R. (2005), Removal of phenol from wastewater using date seed carbon. *Journal of the Chinese Chemical Society*, **52** (6), 1117-1122.
289. Ho, Y.S. (2005), Comments on “Study on biosorption of Cr(VI) by Mucor hiemalis”. *Biochemical Engineering Journal*, **26** (1), 82-83.
290. Chubar, N.I., Samanidou, V.F., Kouts, V.S., Gallios, G.G., Kanibolotsky, V.A., Strelko, V.V. and Zhuravlev, I.Z. (2005), Adsorption of fluoride, chloride, bromide, and bromate ions on a novel ion exchanger. *Journal of Colloid and Interface Science*, **291** (1), 67-74.
291. Ho, Y.S. (2005), Comments on “Efficiency of membrane-sorption integrated processes”. *Journal of Membrane Science*, **263** (1-2), 160-161.
292. Ho, Y.S. (2005), Effect of pH on lead removal from water using tree fern as the sorbent. *Bioresource Technology*, **96** (11), 1292-1296.
293. Blazquez, G., Hernainz, F., Calero, M. and Ruiz-Nunez, L.F. (2005), Removal of cadmium ions with olive stones: the effect of somes parameters. *Process Biochemistry*, **40** (8), 2649-2654.
294. Maity, S., Chakravarty, S., Bhattacharjee, S. and Roy, B.C. (2005), A study on arsenic adsorption on polymetallic sea nodule in aqueous medium. *Water Research*, **39** (12), 2579-2590.
295. Ho, Y.S. (2005), Comment on “Two-stage batch sorber design using second-order kinetic model for the sorption of metal complex dyes onto pine sawdust” by Ozacar,M and Sengyl,IA. *Biochemical Engineering Journal*, **23** (3), 291-292.
296. Ho, Y.S. (2005), Adsorption characteristics of zinc-cyanide complexes by waste brewery biomass. *Journal of Industrial and Engineering Chemistry*, **11** (3), 478-479.
297. Ho, Y.S. (2005), Comment on ‘Biosorption of cadmium using the fungus Aspergillus niger’. by Barros, L.M., Macedo, G.R., Duarte, M.M.L., Silva, E.R and Lobato, A.K.C.L. *Brazilian Journal of Chemical Engineering*, **22** (2), 319-322.
298. Ho, Y.S. (2005), Comment on “Selective adsorption of tannins onto hide collagen fibres”. *Science in China Series B-Chemistry* , **48** (2), 176.
299. Chubar, N.I., Kanibolotskyy, V.A., Strelko, V.V., Gallios, G.G., Samanidou, V.F., Shaposhnikova, T.O., Milgrandt, V.G. and Zhuravlev, I.Z. (2005), Adsorption of phosphate ions on novel inorganic ion exchangers. *Colloids and Surfaces A-Physicochemical and Engineering Aspects*, **255** (1-3), 55-63.
300. Ho, Y.S. (2005), Comment on “Adsorption of naphthalene on zeolite from aqueous solution” by C.F Chang, C.Y. Chang, K.H. Chen, W.T. Tsai, J.L. Shie, Y.H. Chen. *Journal of Colloid and Interface Science*, **283** (1), 274-277.
301. Ho, Y.S. (2005), Comment on “Nitrate removal from aqueous solution by adsorption onto various materials” by N. Ozturk, T.E. Bekta. *Journal of Hazardous Materials*, **118** (1-3), 253-254.
302. Ho, Y.S. (2005), Comments on “Chitosan functionalized with 2[-bis-(pyridylmethyl) aminomethyl]4-methyl-6-formyl-phenol: equilibrium and kinetics of copper(II) adsorption”. *Polymer*, **46** (5), 1451-1452.
303. Psareva, T.S., Zakutevskyy, O.I., Chubar, N.I., Strelko, V.V., Shaposhnikova, T.O., Carvalho, J.R. and Correia, M.J.N. (2005), Uranium sorption on cork biomass. *Colloids and Surfaces A-Physicochemical and Engineering Aspects*, **252** (2-3), 231-236.
304. Ho, Y.S. (2005), Comment on “Removal of heavy metals from aqueous solution by carbon nanotubes: adsorption equilibrium and kinetics” by Li, Y.H., Di, Z.C., Luan, Z. K., Ding, J., Zuo, H., Wu, X. Q., Xu, C. L. and Wu, D. H. *Journal of Environmental Sciences-China*, **17** (1), 175-176.
305. Gawade, A.S., Vanjara, A.K. and Sawant, M.R. (2005), Removal of herbicide from water with sodium chloride using surfactant treated alumina for wastewater treatment. *Separation and Purification Technology*, **41** (1), 65-71.
306. Ofomaja, E.A., Unuabonah, I.E. and Oladoja, N.A. (2005), Removal of lead from aqueous solution by palm kernel fibre. *South African Journal of Chemistry-Suid-Afrikaanse Tydskrif Vir Chemie*, **58**), 127-130.
307. Al-Asheh, S., Banat, F. and Masad, A. (2005), Use of activated oil shale for the removal of 2,4-dichlorophenol from aqueous solutions. *Water Quality Research Journal of Canada*, **40** (2), 211-221.
308. Zheng, S.K., Yang, Z.F., Jo, D.H., Park, Y.H. and Ho, Y.S. (2005), Comment on “Removal of chlorophenols from groundwater by chitosan sorption”. *Water Research*, **39** (1), 264-268.
309. Ho, Y.S. (2004), Comment on “Sorption of basic dyes from aqueous solution by activated sludge” [J. Hazard. Mater. 108 (2004) 183-188]. *Journal of Hazardous Materials*, **114** (1-3), 241-245.
310. Ho, Y.S. (2004), Comments on “collagen-fiber-immobilized tannins and their adsorption of Au(III). *Industrial & Engineering Chemistry Research*, **43** (19), 6265.
311. Sepulveda, L., Fernandez, K., Contreras, E. and Palma, C. (2004), Adsorption of dyes using peat: Equilibrium and kinetic studies. *Environmental Technology*, **25** (9), 987-996.
312. Ho, Y.S. (2004), Comment on “Removal of copper from aqueous solution by aminated and protonated mesoporous aluminas: kinetics and equilibrium,” by S. Rengaraj, Y. Kim, C.K. Joo, and J. Yi. *Journal of Colloid and Interface Science*, **276** (1), 255-258.
313. Ho, Y.S. (2004), “Kinetic modeling and equilibrium studies during cadmium biosorption by dead Sargassum sp biomass” by Cruz, C.C.V.., da Costa, A.C.A., Henriques, C.A., Luna, A.S. *Bioresource Technology*, **93** (3), 321-323.
314. Benaissa, H. and Benguella, B. (2004), Effect of anions and cations on cadmium sorption kinetics from aqueous solutions by chitin: experimental studies and modeling. *Environmental Pollution*, **130** (2), 157-163.
315. Ho, Y.S. (2004), Cadmium removal from aqueous solutions by chitin: kinetic and equilibrium studies. *Water Research*, **38** (12), 2962-2964.
316. Ho, Y.S. (2004), Pseudo-isotherms using a second order kinetic expression constant. *Adsorption-Journal of the International Adsorption Society*, **10** (2), 151-158.
317. Ho, Y.S. (2004), Comment on “Arsenic removal using mesoporous alumina prepared via a templating method”. *Environmental Science & Technology*, **38** (11), 3214-3215.
318. Ho, Y.S., Chiu, W.T., Hsu, C.S. and Huang, C.T. (2004), Sorption of lead ions from aqueous solution using tree fern as a sorbent. *Hydrometallurgy*, **73** (1-2), 55-61.
319. Ho, Y.S. (2004), Comment on “An alternative Avrami equation to evaluate kinetic parameters of the interaction of H9(II) with thin chitosan membranes, by E.C.N. Lopes, F.S.C. dos Anjos, E.F.S. Vieira, and A.R. Cestari. *Journal of Colloid and Interface Science*, **272** (1), 249-250.
320. Ho, Y.S. and Wang, C.C. (2004), Pseudo-isotherms for the sorption of cadmium ion onto tree fern. *Process Biochemistry*, **39** (6), 759-763.
321. Ho, Y.S., Bulut, Y. and Tez, Z. (2004), ‘Removal of heavy metal ions by modified sawdust of walnut’ by Bulut, Y and Tez, Z. *Fresenius Environmental Bulletin*, **13** (4), 370-373.
322. Jadhav, D.N. and Vanjara, A.K. (2004), Removal of phenol from wastewater using sawdust, polymerized sawdust and sawdust carbon. *Indian Journal of Chemical Technology*, **11** (1), 35-41.
323. Ho, Y.S. (2003), Removal of metal ions from sodium arsenate solution using tree fern. *Process Safety and Environmental Protection*, **81** (B5), 352-356.
324. Ho, Y.S. (2003), Affinity dye-ligand poly(hydroxyethyl methacrylate)/chitosan composite membrane for adsorption lysozyme and kinetic properties G. Bayramoglu, M. Yilmaz, M.Y. Arica. *Biochemical Engineering Journal*, **15** (1), 77-78.
325. Ho, Y.S. (2003), Untitled. *Journal of Chemical Technology and Biotechnology*, **78** (6), 724.
326. Ho, Y.S. (2003), Comment on “Adsorption of fluoride, phosphate, and arsenate ions on a new type of ion exchange fiber,” by RX Liu, J.L. Guo, and HX Tang. *Journal of Colloid and Interface Science*, **262** (1), 307-308.
327. Ho, Y.S. (2003), Removal of copper ions from aqueous solution by tree fern. *Water Research*, **37** (10), 2323-2330.
328. Ho, Y.S. (2002), Comment on “Removal of Ni2+ and Cu2+ ions from aqueous solutions on to lignite-based carbons”, by S.E. Samra. *Adsorption Science & Technology*, **20** (2), 199-201.
329. Ho, Y.S., Porter, J.F. and Mckay, G. (2002), Equilibrium isotherm studies for the sorption of divalent metal ions onto peat: Copper, nickel and lead single component systems. *Water Air and Soil Pollution*, **141** (1-4), 1-33.
330. Ho, Y.S. and Chiang, C.C. (2001), Sorption studies of acid dye by mixed sorbents. *Adsorption-Journal of the International Adsorption Society*, **7** (2), 139-147.
331. Ho, Y.S., Chiang, C.C. and Hsu, Y.C. (2001), Sorption kinetics for dye removal from aqueous solution using activated clay. *Separation Science and Technology*, **36** (11), 2473-2488.
332. Reddy, S. and Kotaiah, B. (2006), Comparative evaluation of commercial and sewage sludge based activated carbons for the removal of textile dyes from aqueous solutions. *Iranian Journal of Environmental Health Science & Engineering*, **3** (4), 239-246.
333. Oladoja, N.A., Asia, I.O., Aboluwoye, C.O., Oladimeji, Y.B. and Ashogbon, A.O. (2008), Studies on the sorption of basic dye by rubber (Hevea brasiliensis) seed shell. *Turkish Journal of Engineering and Environmental Sciences*, **32** (3), 143-152.
334. Nayak, P.S., Singh, B.K. and Nayak, S. (2007), Equilibrium, kinetic, and thermodynamic studies on phenol sorption to clay. *Journal of Environmental Protection Science*, **1**, 83-91.
335. Huang, C.T. (2004), Removal of lead ions from aqueous solution by using tree fern. *M.Sc. Thesis*, Taipei Medical University, Taipei, Taiwan.